{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,4,1],[3,2,4,3],[3,4,4,5],[3,6,4,7],[3,8,4,8],[5,0,5,1],[5,2,5,3],[5,4,5,5],[5,6,5,7],[6,0,6,1],[6,2,6,3],[6,4,6,5],[6,6,6,7],[7,0,7,1],[7,2,7,3],[7,4,7,5],[7,6,7,7],[8,0,8,1],[8,2,8,3],[8,4,8,5],[8,6,8,7],[9,0,9,1],[9,2,9,3],[9,4,9,5],[9,6,9,7],[10,0,10,1],[10,2,10,3],[10,4,10,5],[10,6,10,7],[11,0,11,1],[11,2,11,3],[11,4,11,5],[11,6,11,7],[12,0,12,1],[12,2,12,3],[12,4,12,5],[12,6,12,7],[13,0,13,1],[13,2,13,3],[13,4,13,5],[13,6,13,7],[14,0,14,1],[14,2,14,3],[14,4,14,5],[14,6,14,7],[15,0,15,1],[15,2,15,3],[15,4,15,5],[15,6,15,7],[16,0,16,1],[16,2,16,3],[16,4,16,5],[16,6,16,7],[17,0,17,1],[17,2,17,3],[17,4,17,5],[17,6,17,7],[18,0,18,1],[18,2,18,3],[18,4,18,5],[18,6,18,7],[19,0,19,1],[19,2,19,3],[19,4,19,5],[19,6,19,7],[20,0,20,8],[21,0,21,8],[22,0,22,8],[23,0,23,8]],"flags":["formulas_cached_only"]}
["莆田哲理中学教室空调布线工程量清单"]
[""]
["1、工程名称：教室空调布线项目"]
["序号",null,"项目名称",null,"项目特征描述",null,"计量单位",null,"工程量"]
[]
["1",null,"落地式配电箱（伟业牌）",null,"成套配电箱安装 落地式",null,"台",null,3]
["2",null,"配电箱（伟业牌）",null,"成套配电箱安装 悬挂嵌入式(半周长1.0m)  配电箱开关模数 20以内",null,"台",null,18]
["3",null,"普通灯具拆除",null,"电气照明拆除灯具",null,"套",null,88]
["4",null,"普通灯具安装",null,"(1)荧光灯具安装 \r\n(2)不计主材",null,"套",null,88]
["5",null,"开孔（打洞）",null,"(1)室内管道 砖结构 洞口截面100mm×100mm 深(260mm以内)\r\n(2)室内管道 修补洞眼 洞口100mm×100mm 深(300mm以内)",null,"个",null,124]
["6",null,"桥架（大全、泰丰牌）",null,"桥架安装 钢制桥架100*100",null,"m",null,100]
["7",null,"桥架（大全、泰丰牌）",null,"桥架安装 钢制桥架100*50",null,"m",null,1700]
["8",null,"配线（南平太阳牌）",null,"线槽配线 BV-4",null,"m",null,12552]
["9",null,"配线（南平太阳牌）",null,"线槽配线 BV-2.5",null,"m",null,3138]
["10",null,"配线（南平太阳牌）",null,"线槽配线 BV-10",null,"m",null,252]
["11",null,"配线（南平太阳牌）",null,"线槽配线 BV-25",null,"m",null,1240]
["12",null,"电力电缆（南平太阳牌）",null,"铜芯电力电缆敷设 5*50",null,"m",null,35]
["13",null,"电力电缆（南平太阳牌）",null,"铜芯电力电缆敷设 5*90",null,"m",null,28]
["14",null,"塑料管（亚通牌）",null,"室内管道 空调冷凝水塑料管DN40",null,"m",null,380]
["15",null,"刷卡器全套",null,"(1)预付费电表读卡器（含2张卡）380V\r\n(2)需与原空调系统相配套",null,"套",null,88]
["2、投标下浮率：            （至少14%）"]
["3、我单位已与校方总务处联系对该工程进行现场勘察，已清楚布线等所有情况。"]
["4、投标单位：                          （盖章）"]
["2016-06-16"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}